$NOME

Manuale Software

MAREL srl - FABRIANO (AN) – Italy

www.marelsrl.com

Indice generale

Assign IP Address

This procedure explains how to assign an IP address to a Phoenix Contact FL IL BK B PAC device, with the IPAssign.exe utility.

Opening application

Once you opened application, press the Next button. In the next page there are all Phoenix devices found in a list. Check MAC Address correspondence with the one in the label of physical device. If you don't see your device, restart it.

List of devices to configure IP Address

Select your device and press the Next button again. In the next page, configure IP Address and Subnet Mask of the device, and press Next.

IP Address configuration

Internal configuration

You can configure the Phoenix Contact FL IL 24 BK B PAC device with its web interface, using Internet Explorer to navigate in its IP Address.

Web interface

Follow the Inline Station link from the left menu. In the next page, press Disable on Plug & Play Mode box, insert ”private” as password and press Apply to confirm changes.

Web interface - Inline station

Now follow the Process Data Monitoring from the left menu. In the next page, set the Process Data Watchdog Timeout field to ”0 ms”, insert ”private” as password and press Apply to confirm changes.

Web interface - Process data monitoring